# Print settings:

* Print material: PLA
* Rotation of the objects: No comment.
* Support: No
* Skirt, brim: Skirt.
* Infill: 20%

# Additional instructions

* None

# Materials needed

* PLA
* 1 x Bolt M2.5 x 20
* 1 x nuts M2.5

# Log history

# Version 0.3

* The reed contact was not stable, especially not by cold weather around 1’C
* Create a ‘switch holder 01’ and a ‘switch bump 01’ to let the switch wheel run into

# Version 0.2

* Used a larger magnet
* Moved the position of the reed contact to have a closer contact with the magnet

# Version 0.1

* First release